Veda IF91x : Execute to read BDADDR and reset
.
Please be patient for about 3 seconds for Read BDADDR...
...******************************...
...*** DO NOT PRESS ANY KEY ! ***...
...******************************...
..
Auto-detecting BT COM by VID/PID/SN (Prefix=VID_0403+PID_6001, SN=FT90HOHLA)...
Detected RP2040 UART COM port (MI_01): COM29
Detected FTDI/RP2040 COM port -> COM29
Read will use COM29
BT will use COM29
...
.. Bluetooth Read BDADDR / Reset ..
>> ./MbtP.exe COM29 help
>> ./MbtP.exe reset COM29
[HCI] Success pattern matched; ignoring non-zero exit code (1).
>> ./MbtP.exe read_bdaddr COM29
.....
Bluetooth read BDADDR and Reset successfully ...
Done.
