==== IF91x 2.4GHz TX Test (11gn) ====
Veda IF91x : Execute to transmit 2.4GHz Tx 11gn performance
.
Please be patient for about 5 seconds for Transmit Tx...
...******************************...
...*** DO NOT PRESS ANY KEY ! ***...
...******************************...
..
Auto-detecting WL COM by VID/PID/SN (Prefix=VID_0403+PID_6001, SN=FT8EBM6XA)...
Detected FTDI via VID/PID/SN -> COM16
WL will use COM16
Found FTDI device Instance ID:
    FTDIBUS\VID_0403+PID_6001+FT8EBM6XA\0000
[RF] Country=US  PHY=11gn  CH=1  BW=20MHz  Rate=HT-MCS4
...
.. Wi-Fi Transmit Tx 11gn (2.4GHz) ..
>> ./wl_rc1.exe --serial 16 ver
18.15 RC1.0
wl0: Mar  6 2025 05:05:12 version 28.10.400.1 (9de5969 WLTEST) FWID 01-913760f7

>> ./wl_rc1.exe --serial 16 cur_etheraddr
cur_etheraddr E8:CB:F5:C0:00:6A

>> ./wl_rc1.exe --serial 16 pkteng_stop tx
>> ./wl_rc1.exe --serial 16 down
>> ./wl_rc1.exe --serial 16 spect 0
>> ./wl_rc1.exe --serial 16 mpc 0
>> ./wl_rc1.exe --serial 16 phy_watchdog 0
>> ./wl_rc1.exe --serial 16 country US
>> ./wl_rc1.exe --serial 16 band b
>> ./wl_rc1.exe --serial 16 chanspec 1
Chanspec set to 0x1001

>> ./wl_rc1.exe --serial 16 mimo_txbw -1
>> ./wl_rc1.exe --serial 16 up
>> ./wl_rc1.exe --serial 16 phy_forcecal 1
>> ./wl_rc1.exe --serial 16 scansuppress 1
>> ./wl_rc1.exe --serial 16 ldpc_cap 1
>> ./wl_rc1.exe --serial 16 txchain 1
>> ./wl_rc1.exe --serial 16 txcore -s 1 -c 2
>> ./wl_rc1.exe --serial 16 2g_rate -h 4 -b 20
>> ./wl_rc1.exe --serial 16 txpwr1 -o -q 72
>> ./wl_rc1.exe --serial 16 pkteng_start 00:11:22:33:44:55 tx 1000 1024 0
.....
WLAN 2.4GHz Transmit Tx successfully ...
Done.
