.
Veda IF91x : Execute to download the Wi-Fi firmware
Please be patient for about 60 seconds for program WLAN firmware...
...******************************...
...*** DO NOT PRESS ANY KEY ! ***...
...******************************...
..
Detected RP2040 UART COM port (MI_01): COM29
Detected FTDI/RP2040 COM port -> COM29
Program will use COM29
Auto-detect successful -> skipping FTDI fallback logic.
...
.. Wi-Fi Firmware programming ..
.. Push [RECOVERY > RESET] button on chip to autobaud state then press ENTER key! ..
...
.. ** Step.1 ** 
..           Push-hold [RECOVERY] > Press [RESET] > Release [RESET] > Release [RECOVERY]
.. ** Step.2 ** 
..           Press keyboard [ENTER] key
.
.....
Device programmed successfully ...
Done.
