==== IF91x 6GHz UNII-7/8 TX Test (11ax) ====
Veda IF91x : Execute to transmit 6GHz UNII-7/8 Tx 11ax performance
.
Please be patient for about 5 seconds for Transmit Tx...
...******************************...
...*** DO NOT PRESS ANY KEY ! ***...
...******************************...
..
Auto-detecting WL COM by VID/PID/SN (Prefix=VID_0403+PID_6001, SN=FT8EBM6XA)...
Detected FTDI via VID/PID/SN -> COM16
WL will use COM16
Found FTDI device Instance ID:
    FTDIBUS\VID_0403+PID_6001+FT8EBM6XA\0000
[RF] Country=US  PHY=11ax  CH=233  BW=20MHz  Rate=UNII-7/8 HE-MCS0
...
.. Wi-Fi Transmit Tx 11ax (5GHz) ..
>> ./wl_rc1.exe --serial 16 ver
18.15 RC1.0
wl0: Mar  6 2025 05:05:12 version 28.10.400.1 (9de5969 WLTEST) FWID 01-913760f7

>> ./wl_rc1.exe --serial 16 cur_etheraddr
cur_etheraddr E8:CB:F5:C0:00:6A

>> ./wl_rc1.exe --serial 16 pkteng_stop tx
>> ./wl_rc1.exe --serial 16 down
>> ./wl_rc1.exe --serial 16 spect 0
>> ./wl_rc1.exe --serial 16 mpc 0
>> ./wl_rc1.exe --serial 16 up
>> ./wl_rc1.exe --serial 16 down
>> ./wl_rc1.exe --serial 16 isup
0

>> ./wl_rc1.exe --serial 16 band s
>> ./wl_rc1.exe --serial 16 country US
>> ./wl_rc1.exe --serial 16 chanspec 233/20
Chanspec set to 0x90e9

>> ./wl_rc1.exe --serial 16 up
>> ./wl_rc1.exe --serial 16 isup
1

>> ./wl_rc1.exe --serial 16 6g_rate -e 0x1
>> ./wl_rc1.exe --serial 16 pe_ext 0
>> ./wl_rc1.exe --serial 16 frameburst 1
>> ./wl_rc1.exe --serial 16 down
>> ./wl_rc1.exe --serial 16 isup
0

>> ./wl_rc1.exe --serial 16 wd_disable 1
>> ./wl_rc1.exe --serial 16 phy_set_ant 0x10
>> ./wl_rc1.exe --serial 16 spatial_policy 1
>> ./wl_rc1.exe --serial 16 stbc_rx 0
>> ./wl_rc1.exe --serial 16 stbc_tx 0
>> ./wl_rc1.exe --serial 16 ldpc_cap 1
>> ./wl_rc1.exe --serial 16 txcore -o 0x1
>> ./wl_rc1.exe --serial 16 mpc 0
>> ./wl_rc1.exe --serial 16 up
>> ./wl_rc1.exe --serial 16 isup
1

>> ./wl_rc1.exe --serial 16 txpwr1 -o -q 60
>> ./wl_rc1.exe --serial 16 phy_watchdog 0
>> ./wl_rc1.exe --serial 16 up
>> ./wl_rc1.exe --serial 16 phy_forcecal 1
>> ./wl_rc1.exe --serial 16 phy_activecal 1
>> ./wl_rc1.exe --serial 16 longpkt 1
>> ./wl_rc1.exe --serial 16 interference_override 0
>> ./wl_rc1.exe --serial 16 pkteng_start 00:11:22:33:44:55 tx 1000 1024 0
>> ./wl_rc1.exe --serial 16 phy_tempsense
28

.....
WLAN 6GHz UNII-7/8 Transmit Tx successfully ...
Done.
