[5591x image download]

1. copy these files to this folder
(in the path: cyw55913-mfg-unified-app-master\build\APP_CYW955913EVK-01\Release\ )
minidriver.hex
wifi-unified-tester.btp
wifi-unified-tester_download.hcd/wifi-unified-tester_download.hex

2. power on EVB and switch to download mode.

3. check com port number (HCI uart port)

4. run downaload.bat
command:  downaload.bat [COM port number]

example:  download.bat 3



## 5591x_IMG_V300.zip ##
firmware - V3.0.0
NVram - original


## 5591x_IMG_V301.zip ##
firmware - V3.0.1
NVram - ASE3.0.1

